1. W/L CONFERENCE EQUIPMENT CENTRAL UNIT

모델 : TOA, TS-920RC

(1) 기  능

본 기기는 무선 적외선 회의 시스템의 중앙 장치로 쉬운 설치와 유연한 배치가 가능하여야한다. TS-905/907 IR 송신기/수신기를 연결함으로써 무선 적외선 신호를 통해 의장 및 의원 장치를 제어 할 수 있어야한다. IR송신기/수신기 및 의장/의원 장치의 연결 상태를 확인할 수 있는 설치 확인 기능이 가능하여야한다. FBS(피드백 억제기)도 장착되어 있어 음향 피드백을 효과적으로 제어가 가능하여야한다. MP3 레코더 내장 되어있어 USB 메모리 또는 내부 메모리에 모든 회의 내용을 기록 가능한 기기로 다음과 같은 규격에 준한다.

(2) 성  능

- Power Source : 100 - 240V ac, 50/60 Hz

- Power Consumption : 72W

- Current Consumption : 3A DC

- Carrier Frequency : Reception : Audio channel 1: 7.35MHz

Audio channel 2: 8.10MHz

Audio channel 3: 8.55MHz

Audio channel 4: 9.15MHz

Control channel : 6.45MHz

Transmission : Base Language channel : 1.95MHz

Translation Language Channel : 2.25MHz

- Input : MIC1 : -60 dB, 600 Ω, unbalanced, Ø 6.3mm phone jack (2P)

MIC2 : -60 dB, 600 Ω, unbalanced, Ø 6.3mm phone jack (2P)

AUX1 : -20 dB, 10 kΩ, unbalanced, Ø 6.3mm phone jack (2P)

AUX2 : -20 dB, 10 kΩ, unbalanced, Ø 6.3mm phone jack (2P)

AUX3 : -20 dB, 10 kΩ, unbalanced, Ø 6.3mm phone jack (2P)

- Output : LINE: -10dB, 10kΩ, unbalanced, Ø6.3mm phone jack(2P)

REC: -10dB, 10kΩ, unbalanced, RCA pin jack

HEADPHONES: Ø3.5mm mini jack (3P:monaural)

- Equalizer Input/Output : Input : -20dB, 10kΩ, unbalanced, RCA pin jack

Output : -20dB(x2), 10kΩ, unbalanced, RCA pin jack

- Number of Connectable Infrared Transmitter / Receiver Unit : Up to 4 units

- Number of Connectable Chairman/Delegate Units : 192unit

- Infrared Transmitter/Receiver I/O Terminal : BNC jacks

- External Control Connection Terminal : D-sub connector (9P, male)/	USB-B selectable

- Record Switch : Recording start button, Recording stop button, Format button

- Recording Port : USB-A (for USB memory devices) and USB Mini-B (for PCs)

- Recording Function : Recordings can be made to a USB memory device or                                 the internal memory.

Recording format : MP3 (MPEG-1 Audio Layer-3),                                monaural Sampling frequency : 32kHz, Bit rate : 128 kbps

- Function Switch : Number of open microphones setting switch : 1/2/3/4

Mic-off setting switch : TIME OUT ON/OFF

Speech priority selector switch :

FIRST  (First-in-first-out priority)

LATEST (Last-in-first-out priority)

FIRST : FIXED

NEXT : LATEST (Priority fixed for the first unit, and

last-in-first-out priority for all other subsequent

units)

FBS switch: AUTO/OFF/EXT

- Operating Humidity : 90% RH or less

- Operating Temperature : 0°C to +40°C(32°F to 104°F)

- Finish : Surface-treated steel plate, black, 30 % gloss, paint

- Dimensions : 361(W) x 122.6(H) x 184.2(D)mm

- Weight : 2.8Kg

- 동등 또는 이상 품이어야 한다.